**Elmore County Public Schools**

December 17, 2012

**Bid# 12-005 "72 Passenger Buses"**

Sealed bids for **"72 Passenger Buses"** for use in Elmore County Schools will be received by the

Elmore County Board of Education at its Central Office in Wetumpka until 9:00 a.m., Monday,

January 14, 2013, at which time they will be publicly opened and read.

You may access this bid from our web page www.elmoreco.com under Transportation,

Document Downloads. If you would like to request a hard copy of this bid, you may call 334-567-1229.

The specifications and bid information should be read carefully. On the final page, you must

enter your bid, sign, and have notarized. If the document is not submitted as requested, it may be

such that we cannot classify this offer as a legitimate bid.

The bid will be awarded to the responsible bidder(s) offering the proposal(s) deemed the most

acceptable and advantageous to the System. The Elmore County Board of Education reserves the

right to reject any/and/or all bids and to waive informalities in awarding this bid to the lowest

responsible bidder.

Any questions that may arise concerning bid procedure and technical information, must be

submitted in writing to the writer, Dr. Robert Slater, Transportation Supervisor, Elmore County Public Schools, PO Box 817, 100 H.H. Robinson Drive, Wetumpka, AL 36092. Any changes, additions, modifications to the bid request will be posted to the Elmore County School System website at

[www.elmoreco.com](http://www.elmoreco.com). *It is the responsibility of the vendor to check the website on a daily*

*basis for any changes to the bid request.* No changes will be made as of 48 hours prior to bid

opening.

Sincerely,

Robert Slater, Ph.D.

Transportation Supervisor

Elmore County Public Schools

**2012 BID #12-005**

**72 PASSENGER SCHOOL BUSES**

BIDDERS ARE REQUESTED TO RETAIN THESE INSTRUCTIONS, CONDITIONS, AND SPECIFICATIONS FOR FUTURE REFERENCE. ONCE AWARDED THIS IS YOUR CONTRACT DOCUMENT.

I. GENERAL INFORMATION

(A) All bidders must use our form for submitting their bid.

(B) All bids must be sealed and marked in the lower left hand comer "SCHOOL BUS BID" with bid number, opening time and date. Late bids will not be opened.

(C) Bids will not include State Sales Tax, Federal Excise Taxes or any other fee.

(D) Records showing successful bidder(s) and prices quoted will be placed on file and may be examined upon request. If the contract is awarded to someone other than lowest bidder, a note of explanation will appear in the bid file.

(E) Use of trade names and numbers shall be interpreted as establishing a standard of quality and shall not be construed as limiting competition.

(F) It is the responsibility of the vendor to secure a copy of the Alabama Minimum Specifications For School Buses for 2013 from the Division of Administration and Financial/Pupil Transportation Section/Department of Education, Montgomery, Alabama 36130.

(G) In accordance with the Alabama State Bid Law 3% rule, preference will be given to resident bidders from the Standard Metropolitan Statistical Area.

II. DISQUALIFICATION OF BIDS

Bids may be disqualified before the awarding of the contract for any of the following:

(A) Failure to mark envelope as required.

(B) Failure to sign or notarize the bid document.

(C) Failure to include requested information or other details of the bid.

(D) Excessive errors.

(E) Failure to have an original signature on the bid form, a faxed copy is not acceptable.

III. METHOD OF AWARD

(A) The award will be made to the lowest responsible bidder(s) meeting specifications. It is not the policy of the Elmore County Board of Education to purchase on the basis of low bid only. Quality, conformity within Specifications, purpose for which required, terms of delivery, past service and experience are among the factors that may be considered in determining the responsible bidder.

(B) In the event the low bidder refuses to accept the entire requirements without deviation, the bid may be awarded to the next lowest bidder.

(C) In the event that two or more vendors bid the same amount on the same item, a coin toss will determine the vendor awarded that item.

(D) The Elmore County Board of Education reserves the right to have any chassis/body offered for bid inspected by their representative prior to the selection of that vendor.

(E) The Elmore County Board of Education reserves the right to award separate contracts for each item, each product, or any combination of products, if the Board feels it is in the best interest of the Elmore County Public School System

IV. CONTRACT PERIOD/PRICING

(A) If other State or Local Funds become available, the Board may elect to purchase additional chassis/bodies from this bid.

(B) Bid prices should be good for 90 days. Effective date of bid will begin immediately after being awarded.

(C) May be extended for two additional 90-day periods. The extension must have the mutual consent of the vendor and the Elmore County Board of Education. All terms and prices must remain the same.

(D) Prices should include delivery to Wetumpka, Alabama.

V. QUANTITIES/ORDERS/DELIVERIES

(A) **The original Purchase Order will be placed on or after January 14, 2013 for approximately: 1 or more - 72 passenger bus chassis/body equipped with diesel motor**

(B) Quantities are estimates only. Actual purchases may be more or less depending on funds available.

(C) Number of days required for delivery must be stated and will become a part of the terms of this bid contract.

**The only exception to the extension of the contract date will be general strikes at the chassis/body plants and acts of God.**

(D) Before the order is placed, there will be a meeting with the successful vendor to make sure all specs are understood and clarified.

(E) At the time the buses are delivered, the vendor(s) must supply a 4-wheel alignment data sheet for each bus.

VI. WARRANTIES/SERVICE

(A) All warranties must be clearly stated.

(B) Availability of service must be clearly stated along with service contract pricing. Service centers with times and days of operation must be stated. If road service is provided, it must be noted.

VII. SPECIFICATIONS

All bids must have attached printed specifications (unless a sample is already on file with the Elmore County Board of Education), showing a photograph or drawing of the item bid. All Chassis must meet Federal Motor Vehicle Safety Standards and the 2013 Minimum Alabama State Specifications for School Buses. It is the responsibility of the vendor to secure these specifications.

**PLEASE MAIL BID TO THE FOLLOWING ADDRESS:**

**Elmore County Board of Education**

**Bid #12-005** "**72 Passenger School Buses"**

**P.0. Box 817 (100 H.H. Robinson Drive, if hand delivered)**

**Wetumpka, AL 36092**

**All vehicles must be delivered to the Elmore County Schools Transportation Department as per specifications by 12:00 p.m. on 7/1/2013. Any vehicle not meeting this deadline will be assessed $100.00 per vehicle per day.**

**CHASSIS DATA:**

1. Air brake compressor to be 18.7 CFM. Duel full service s-cam brakes 5” front and 7” rear, 7/8” thick extended service.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Alternator to be a 185 amp minimum. (Bosch or Delco preferred)

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Axles: Front, 10,000 lbs. Rear, 21,000 lbs. minimum. Air ride rear suspension.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Batteries (2) need to be Group 31 with a minimum total of 1850 CCA, mounted in a heavy duty roll out tray compartment. (Deka batteries preferred)

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Radiator, aluminum with long life coolant to -40 degrees.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

6. Engine: diesel 220 HP minimum. Engine must be inline six cylinder to include 5 yr. 100,000 mile minimum parts (including sensors) and labor warranty. Warranty to include all electronics, injectors, and major components. Copy of warranty to be included with bid. Exhaust pipe must exit the rear of the bus. Engine must be either an International or Cummins

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Transmission to be Allison PTS 2500. First fill synthetic fluid with a 5 year unlimited mile warranty.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Drive Line, Spicer “Lube for Life” or equal and dynamically balanced.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Fuel tank, 100 gallons mounted between the frame rails. Locking fuel tank door and fuel water separator.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Instrument panel gauges to include speed odometer, reset trip odometer, voltmeter, low air dual gauges with warning light buzzer, tachometer, digital clock, cruise control and hour meter.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Factory must set idle time at 5 minutes and must be adjustable by Elmore County Shop Personnel.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Headlights must be long life halogen or better with daytime running lights.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Tires to be Continental HSR, Goodyear, Bridgestone, or approved equal, 11R x 22.5 14 ply radials. Wheels to be budd type, hub pilot and painted black.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Steering column to be tilt.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Tow hooks, front and rear, mounted to frame rails.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Turning, at least a 50 degree wheel cut.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Easy tilt hood assist, less than 15 lbs. of opening effort.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Chassis, electric heater water booster pump. Pump must be non-plastic and serviceable.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

19. Electronic governor to allow not more than 65 mph maximum. Speed must be adjustable by Elmore County Shop Personnel.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 20. Filler tube for fuel tank must be on right side of bus

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 21. Each chassis must be equipped with both spare tire and rim – 11 x 22.5 Hwy tread (Continental HSR, Goodyear, or Bridgestone)

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 22. Do not install dust covers on front and rear brakes.

 Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 23. Chassis must be current year or newer.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 24. Removable access panel for access to rear of engine.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**BODY DATA:**

1. Body must have four applied rub rails on each side and painted black.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Heavy duty rubber floor covering under seats. Molded rubber over wheel housing.

 Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Interior headroom to be 77” min.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Heating system to include a minimum 90,000 BTU front left heater and defroster, 50,000 BTU min. right entrance door heater and 50,000 BTU rear under seat heater.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Dual 6” defroster driver’s fans, one mounted in the center and one over driver’s window above driver.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Must have perforated acoustical headliner (front to rear), minimum ceiling height of 77”.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Driver’s seat to be air ride, manufacturer’s standard with vinyl and cloth insert upholstery.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Driver’s seat belt to be 3-point with vertical adjustment. Orange.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Passenger seats to be manufacturer’s standard. Color to be gray.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. The roof shall be painted white. All paint including base, trim and roof shall be heat cured or equal.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Stop arm and crossing gate shall be air operated. Stop arm must be L.E.D. Strobe.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Unit must have dome lights, ceiling mounted, plus a driver’s dome light.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Exterior mirrors, outside rearview mirrors must be Rosco, open view, split system. Crossview mirrors must be Rosco, Eye-Max-LP or equal.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Unit shall have all side passenger windows tinted to 28% transmission in aluminum frames. Entrance door and driver’s windows are green tint.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Assist rail on both left and right, located in the passenger entry.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Units must have armored protective clearance and cluster lights.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Each bus shall be equipped with a body and chassis specific line setting ticket with a complete list of parts by quantity, parts number and description in order to accurately facilitate parts replacement. Two parts and service manuals or CD included. (CD preferred)

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. All units must be keyed alike.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Two Specialty roof emergency exits.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. All wiring must be in a loom and have rubber grommet where wires go through body.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Battery, master kill switch to be located in locking battery compartment.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. All lights on the outside of the bus body must be LED. This includes the 8 way, stop, tail, brake, directional, back and side, back-up, clearance, stop sign, cluster and tag lights.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

23. All LED lights must have a minimum 5 year warranty.

 24. All 8 way warning lights must be hooded.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 25. Entrance door preferred to be manual/air operated and equipped with an exterior handle. Electric not

 desired.

Exception\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 26. Body must be current year or newer.

 Exception\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 27. Factory installed power source socket, 12 volt D.C. mounted in drivers' compartment.

 Exception\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 28. Intermittent wipers

Exception\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 29. All numbers and lettering to be completed before delivery.

Exception\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

30. Locking storage compartment in bulkhead as per State specs. Section VI – Options

 Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

31. Locking storage compartments for emergency equipment, electrical panel, fuel door (if provided), and

any other locking compartments must be keyed alike. The same key must open all doors.

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

32. AngelTrax Hybrid Quest- 4 channel mobile DVR with Standard 320g hard drive; 4 RC2500 cameras placement as follows- 1 driver well camera , 2 placed down side of bus to see down into high back seats, 1 placed rear of bus; GPS-E1

Exception:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 33. Adjustable accelerator and brake pedals for the driver

 34. Factory Installed Child Check Safety System

 35. Buses must be State inspected and pass on-site inspection before being accepted.

 No Exception

**ELMORE COUNTY BOARD OF EDUCATION**

**72 Passenger price per unit $\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

Company Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Phone Number:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Fax:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Print Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Days required for delivery \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Units must meet and exceed all Federal and State specifications for school buses.**