Central Office Awning Replacement & Addition (RFP 21-018)

Material specification shall be as follows;

* Columns shall be 4"x4", .125” extruded aluminum and have integrated gutters
* Decking shall be 3"x6", .060" cap and pan extruded aluminum
* Beams shall be 4"x6", .093" extruded aluminum
* Gutter shall be 4"x6", .093" extruded aluminum
* All columns shall be cored and poured into the existing concrete
* Color shall be dark bronze; baked enamel